

Captions

Dallmer\_refurbishment\_new\_building\_object\_01.jpg

Ideal for bathroom renovations with low installation heights: flat floor drains such as the DallFlex Plan.

Photo: Dallmer GmbH + Co KG



Dallmer\_DallFlex\_2.0\_02.

The Connect active drainage system with integrated pump offers the solution to the slope problem and saves on costly pipe renovation.

Photo: Dallmer GmbH + Co KG



Dallmer\_refurbishment\_new\_building\_object\_03.jpg

Preventive fire protection is particularly important in public buildings, in the tourism and healthcare sectors and in residential construction.

Photo: Dallmer GmbH + Co KG



Dallmer\_refurbishment\_new\_building\_object\_04.jpg

Changing building standards and legal requirements for energy saving require higher floor structures. Specially developed for 115 mm installation height: the DallFlex 115 floor drain.

Photo: Dallmer GmbH + Co KG



Dallmer\_refurbishment\_new\_building\_object\_05.jpg

Dallmer has responded to the trend towards ever thinner tiles with the new tileable shower channel CeraFloor Individual Neo.

Photo: Dallmer GmbH + Co KG



Dallmer\_refurbishment\_new\_building\_object\_06.jpg

As a counterpart to the CeraFloor Individual Neo positioned in the shower area, the CeraWall Individual Neo offers a perfect wall-mounted solution.

Photo: Dallmer GmbH + Co KG



Dallmer\_refurbishment\_new\_building\_object\_07.jpg

The new bituminous sleeves protect against capillary moisture on floor drains in the area of components in contact with the ground

Photo: Dallmer GmbH + Co KG